{"text_format":"1","workbook":"xlsx","n_sheets":17,"sheets":["Home","About","Angles","nex7_2_1","nex21_4_1","nex28_4_2","nex49_5_3","nex49_7_0","nex63_6_3","nex84_8_2","nex91_5_6","nex91_9_1","nex112_8_4","nex133_9_4","nex133_11_1","nex147_7_7","nex147_11_2"],"not_rendered":{"charts":0,"images":34,"macros":1,"external_links":0,"defined_names":14,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Home","index":0,"n_rows":18,"n_cols":2,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
[]
[1,"Home"]
[2,"About"]
[3,"Angles"]
[4,"nex7_2_1"]
[5,"nex21_4_1"]
[6,"nex28_4_2"]
[7,"nex49_5_3"]
[8,"nex49_7_0"]
[9,"nex63_6_3"]
[10,"nex84_8_2"]
[11,"nex91_5_6"]
[12,"nex91_9_1"]
[13,"nex112_8_4"]
[14,"nex133_9_4"]
[15,"nex133_11_1"]
[16,"nex147_7_7"]
[17,"nex147_11_2"]

{"sheet":"About","index":1,"n_rows":25,"n_cols":2,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["Raw rotegrity / nexorade data and visuals provided by Adrian Rossiter's Antiprism software"]
["Adrian developed a new ultra fast algorithm to get quick results on nexorades."]
["visit :","http://www.antiprism.com/"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Calculations carried out 15 digit limit."]
["Up to 12 digits  confirmed those data by other parties / other methods."]
[]
["Big thanx to Chris Kitrick, who helped me along nexorade geometry,"]
["and the people of geodesichelp group like TaffGoch, Bryan L, Gerry from Quebec and few more."]
["Me just transformed those numbers to some easier to read (for me) format."]
[]
["Wish you all happy modelling and building."]
["Likhanecz Levente from Hungary."]
[]
["Found some mistake? Drop a mail to:"]
["likhanecz@gmail.com"]

{"sheet":"Angles","index":2,"n_rows":6,"n_cols":1,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["In case you wanna calculate angles between struts."]
["Check on the graphic what colors the 3 struts forming a triangle."]
["Copy/paste the corresponding central angles as a,b,c"]
["Then A,B,C angles calculated on all sheet locally."]
["(central angles and chord lengths refers to 1/3 of a colored band - node to node)"]
["to get proper angles there is a x2 in formulas as each side consist of 2 pieces"]

{"sheet":"nex7_2_1","index":3,"n_rows":15,"n_cols":11,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["geo_1 = nex_7_(2,1) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,26.140549500762912,0.45229194967792102,90,{"$f":"F3/3","v":30},null,{"$f":"RADIANS(D3)*Radius","v":456.23865706887278},{"$f":"E3*Radius","v":452.29194967792102}]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",26.140549500762912,{"$f":"DEGREES(ACOS((COS(RADIANS(I13*2))-COS(RADIANS(I14*2))*COS(RADIANS(I15*2)))/(SIN(RADIANS(I14*2))*SIN(RADIANS(I15*2)))))","v":67.692886935831524},"A"]
[null,null,null,null,null,null,null,"b",26.140549500762912,{"$f":"DEGREES(ACOS((COS(RADIANS(I14*2))-COS(RADIANS(I15*2))*COS(RADIANS(I13*2)))/(SIN(RADIANS(I15*2))*SIN(RADIANS(I13*2)))))","v":67.692886935831524},"B"]
[null,null,null,null,null,null,null,"c",26.140549500762912,{"$f":"DEGREES(ACOS((COS(RADIANS(I15*2))-COS(RADIANS(I13*2))*COS(RADIANS(I14*2)))/(SIN(RADIANS(I13*2))*SIN(RADIANS(I14*2)))))","v":67.692886935831524},"C"]

{"sheet":"nex21_4_1","index":4,"n_rows":14,"n_cols":11,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["geo_1_1 = nex_21_(4,1) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,14.49559614133126,0.25232169076595756,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":252.99587970561578},{"$f":"E3*Radius","v":252.32169076595756}]
[199,255,26,16.289240170644693,0.28334437456819478,90,{"$f":"F4/3","v":30},null,284.30087362587284,283.34437456819478]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",14.49559614133126,{"$f":"DEGREES(ACOS((COS(RADIANS(I12*2))-COS(RADIANS(I13*2))*COS(RADIANS(I14*2)))/(SIN(RADIANS(I13*2))*SIN(RADIANS(I14*2)))))","v":58.172482483059703},"A"]
[null,null,null,null,null,null,null,"b",14.49559614133126,{"$f":"DEGREES(ACOS((COS(RADIANS(I13*2))-COS(RADIANS(I14*2))*COS(RADIANS(I12*2)))/(SIN(RADIANS(I14*2))*SIN(RADIANS(I12*2)))))","v":58.172482483059703},"B"]
[null,null,null,null,null,null,null,"c",16.289240170644693,{"$f":"DEGREES(ACOS((COS(RADIANS(I14*2))-COS(RADIANS(I12*2))*COS(RADIANS(I13*2)))/(SIN(RADIANS(I12*2))*SIN(RADIANS(I13*2)))))","v":70.719750979637169},"C"]

{"sheet":"nex28_4_2","index":5,"n_rows":14,"n_cols":11,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["geo_2 = nex_28_(4,2) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,12.206710919873618,0.21264460677229249,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":213.04729639094037},{"$f":"E3*Radius","v":212.64460677229249}]
[199,255,26,13.904045272698077,0.24207635878141762,180,{"$f":"F4/3","v":60},null,242.67136935493431,242.07635878141761]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",12.206710919873618,{"$f":"DEGREES(ACOS((COS(RADIANS(I12*2))-COS(RADIANS(I13*2))*COS(RADIANS(I14*2)))/(SIN(RADIANS(I13*2))*SIN(RADIANS(I14*2)))))","v":56.94928850601535},"A"]
[null,null,null,null,null,null,null,"b",12.206710919873618,{"$f":"DEGREES(ACOS((COS(RADIANS(I13*2))-COS(RADIANS(I14*2))*COS(RADIANS(I12*2)))/(SIN(RADIANS(I14*2))*SIN(RADIANS(I12*2)))))","v":56.94928850601535},"B"]
[null,null,null,null,null,null,null,"c",13.904045272698077,{"$f":"DEGREES(ACOS((COS(RADIANS(I14*2))-COS(RADIANS(I12*2))*COS(RADIANS(I13*2)))/(SIN(RADIANS(I12*2))*SIN(RADIANS(I13*2)))))","v":71.09597494206804},"C"]

{"sheet":"nex49_5_3","index":6,"n_rows":14,"n_cols":11,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["geo_2_1 = nex_49_(5,3) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,8.8214008596339308,0.15381046819638364,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":153.96248963887024},{"$f":"E3*Radius","v":153.81046819638362}]
[26,255,137,10.203231687907635,0.1778447739584193,180,{"$f":"F4/3","v":60},null,178.07998729780675,177.8447739584193]
[26,88,255,10.298823644695208,0.17950649702277799,90,30,null,179.74838168217403,179.50649702277798]
[199,255,26,10.323238018335523,0.17993088437936017,180,60,null,180.17449288700962,179.93088437936018]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",8.8214008596339308,{"$f":"DEGREES(ACOS((COS(RADIANS(I12*2))-COS(RADIANS(I13*2))*COS(RADIANS(I14*2)))/(SIN(RADIANS(I13*2))*SIN(RADIANS(I14*2)))))","v":55.533618767734382},"A"]
[null,null,null,null,null,null,null,"b",8.8214008596339308,{"$f":"DEGREES(ACOS((COS(RADIANS(I13*2))-COS(RADIANS(I14*2))*COS(RADIANS(I12*2)))/(SIN(RADIANS(I14*2))*SIN(RADIANS(I12*2)))))","v":55.533618767734382},"B"]
[null,null,null,null,null,null,null,"c",10.203231687907635,{"$f":"DEGREES(ACOS((COS(RADIANS(I14*2))-COS(RADIANS(I12*2))*COS(RADIANS(I13*2)))/(SIN(RADIANS(I12*2))*SIN(RADIANS(I13*2)))))","v":71.530177924977281},"C"]

{"sheet":"nex49_7_0","index":7,"n_rows":14,"n_cols":11,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["geo_1_2 = nex_49_(7,0) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,8.8214008596339504,0.15381046819638361,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":153.96248963887058},{"$f":"E3*Radius","v":153.8104681963836}]
[26,255,137,10.20323168790763,0.1778447739584193,180,{"$f":"F4/3","v":60},null,178.07998729780664,177.8447739584193]
[26,88,255,10.29882364469524,0.17950649702277824,90,30,null,179.74838168217457,179.50649702277823]
[199,255,26,10.323238018335514,0.17993088437936022,180,60,null,180.17449288700948,179.93088437936024]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",10.20323168790763,{"$f":"DEGREES(ACOS((COS(RADIANS(I12*2))-COS(RADIANS(I13*2))*COS(RADIANS(I14*2)))/(SIN(RADIANS(I13*2))*SIN(RADIANS(I14*2)))))","v":60.390668953901688},"A"]
[null,null,null,null,null,null,null,"b",10.29882364469524,{"$f":"DEGREES(ACOS((COS(RADIANS(I13*2))-COS(RADIANS(I14*2))*COS(RADIANS(I12*2)))/(SIN(RADIANS(I14*2))*SIN(RADIANS(I12*2)))))","v":61.307333682301334},"B"]
[null,null,null,null,null,null,null,"c",10.323238018335514,{"$f":"DEGREES(ACOS((COS(RADIANS(I14*2))-COS(RADIANS(I12*2))*COS(RADIANS(I13*2)))/(SIN(RADIANS(I12*2))*SIN(RADIANS(I13*2)))))","v":61.545582665167977},"C"]

{"sheet":"nex63_6_3","index":8,"n_rows":14,"n_cols":11,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["geo_3 = nex_63_(6,3) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,7.5945378099784664,0.13245267704227348,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":132.5496899513237},{"$f":"E3*Radius","v":132.45267704227348}]
[26,255,137,8.8216258122016953,0.15381438273135822,180,{"$f":"F4/3","v":60},null,153.96641580183854,153.81438273135822]
[199,255,26,8.970136593245206,0.15639857809039487,90,30,null,156.55841790575619,156.39857809039486]
[26,88,255,9.0977670949468266,0.15861923171342143,360,120,null,158.7859903864217,158.61923171342144]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",8.8216258122016953,{"$f":"DEGREES(ACOS((COS(RADIANS(I12*2))-COS(RADIANS(I13*2))*COS(RADIANS(I14*2)))/(SIN(RADIANS(I13*2))*SIN(RADIANS(I14*2)))))","v":58.828977390961207},"A"]
[null,null,null,null,null,null,null,"b",9.0977670949468266,{"$f":"DEGREES(ACOS((COS(RADIANS(I13*2))-COS(RADIANS(I14*2))*COS(RADIANS(I12*2)))/(SIN(RADIANS(I14*2))*SIN(RADIANS(I12*2)))))","v":61.825963491440213},"B"]
[null,null,null,null,null,null,null,"c",9.0977670949468266,{"$f":"DEGREES(ACOS((COS(RADIANS(I14*2))-COS(RADIANS(I12*2))*COS(RADIANS(I13*2)))/(SIN(RADIANS(I12*2))*SIN(RADIANS(I13*2)))))","v":61.825963491440213},"C"]

{"sheet":"nex84_8_2","index":9,"n_rows":14,"n_cols":11,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["geo_2_2 = nex_84_(8,2) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,6.4081090756854957,0.11178431909792451,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":111.84260219764241},{"$f":"E3*Radius","v":111.78431909792451}]
[248,26,255,7.4694524283963322,0.1302742396431095,180,{"$f":"F4/3","v":60},null,130.36653819660199,130.2742396431095]
[199,255,26,7.7477529997400794,0.13512079670888055,360,120,null,135.22379947673176,135.12079670888056]
[26,88,255,7.8009738826953265,0.13604753942376796,180,60,null,136.15267911511935,136.04753942376797]
[26,255,137,7.9538778503188459,0.13870991373841229,180,60,null,138.82135678951258,138.7099137384123]
[]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",7.4694524283963322,{"$f":"DEGREES(ACOS((COS(RADIANS(I12*2))-COS(RADIANS(I13*2))*COS(RADIANS(I14*2)))/(SIN(RADIANS(I13*2))*SIN(RADIANS(I14*2)))))","v":58.232823450031191},"A"]
[null,null,null,null,null,null,null,"b",7.7477529997400794,{"$f":"DEGREES(ACOS((COS(RADIANS(I13*2))-COS(RADIANS(I14*2))*COS(RADIANS(I12*2)))/(SIN(RADIANS(I14*2))*SIN(RADIANS(I12*2)))))","v":61.776517511727988},"B"]
[null,null,null,null,null,null,null,"c",7.7477529997400794,{"$f":"DEGREES(ACOS((COS(RADIANS(I14*2))-COS(RADIANS(I12*2))*COS(RADIANS(I13*2)))/(SIN(RADIANS(I12*2))*SIN(RADIANS(I13*2)))))","v":61.776517511727988},"C"]

{"sheet":"nex91_5_6","index":10,"n_rows":15,"n_cols":11,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["geo_3_1 = nex_91_(5,6) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,6.108002063134494,0.1065542740024258,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":106.60474672030348},{"$f":"E3*Radius","v":106.5542740024258}]
[26,88,255,7.1252204303851689,0.12427843812329208,180,{"$f":"F4/3","v":60},null,124.35855644058861,124.27843812329208]
[248,26,255,7.4165235449383289,0.1293524043110281,180,60,null,129.44275491085546,129.3524043110281]
[199,255,26,7.4201756582367731,0.12941601219183266,180,60,null,129.5064963125692,129.41601219183266]
[26,255,137,7.4520767666781715,0.12997161967160747,180,60,null,130.06327568990736,129.97161967160747]
[197,255,128,7.6168053101775604,0.13284046252106427,90,30,null,132.93833114598638,132.84046252106427]
[255,154,128,7.6350615809270748,0.13315838924464388,180,{"$f":"F9/3","v":60},null,{"$f":"RADIANS(D9)*Radius","v":133.25696317970096},{"$f":"E9*Radius","v":133.15838924464387}]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",7.6168053101775604,{"$f":"DEGREES(ACOS((COS(RADIANS(I13*2))-COS(RADIANS(I14*2))*COS(RADIANS(I15*2)))/(SIN(RADIANS(I14*2))*SIN(RADIANS(I15*2)))))","v":62.201027421752784},"A"]
[null,null,null,null,null,null,null,"b",7.4520767666781715,{"$f":"DEGREES(ACOS((COS(RADIANS(I14*2))-COS(RADIANS(I15*2))*COS(RADIANS(I13*2)))/(SIN(RADIANS(I15*2))*SIN(RADIANS(I13*2)))))","v":59.985260352287987},"B"]
[null,null,null,null,null,null,null,"c",7.4165235449383289,{"$f":"DEGREES(ACOS((COS(RADIANS(I15*2))-COS(RADIANS(I13*2))*COS(RADIANS(I14*2)))/(SIN(RADIANS(I13*2))*SIN(RADIANS(I14*2)))))","v":59.525907189933982},"C"]

{"sheet":"nex91_9_1","index":11,"n_rows":15,"n_cols":11,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["geo_1_3 = nex_91_(9,1) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,6.1080020631344878,0.10655427400242576,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":106.60474672030337},{"$f":"E3*Radius","v":106.55427400242576}]
[26,88,255,7.1252204303851574,0.12427843812329208,180,{"$f":"F4/3","v":60},null,124.35855644058842,124.27843812329208]
[248,26,255,7.4165235449383307,0.1293524043110281,180,60,null,129.44275491085548,129.3524043110281]
[199,255,26,7.4201756582367828,0.12941601219183266,180,60,null,129.50649631256937,129.41601219183266]
[26,255,137,7.4520767666781715,0.12997161967160745,180,60,null,130.06327568990736,129.97161967160744]
[197,255,128,7.6168053101775737,0.13284046252106427,90,30,null,132.93833114598664,132.84046252106427]
[255,154,128,7.6350615809270801,0.1331583892446441,180,60,null,{"$f":"RADIANS(D9)*Radius","v":133.25696317970105},{"$f":"E9*Radius","v":133.1583892446441}]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",7.1252204303851574,{"$f":"DEGREES(ACOS((COS(RADIANS(I13*2))-COS(RADIANS(I14*2))*COS(RADIANS(I15*2)))/(SIN(RADIANS(I14*2))*SIN(RADIANS(I15*2)))))","v":57.946534212748418},"A"]
[null,null,null,null,null,null,null,"b",7.4165235449383307,{"$f":"DEGREES(ACOS((COS(RADIANS(I14*2))-COS(RADIANS(I15*2))*COS(RADIANS(I13*2)))/(SIN(RADIANS(I15*2))*SIN(RADIANS(I13*2)))))","v":61.81682820230494},"B"]
[null,null,null,null,null,null,null,"c",7.4201756582367828,{"$f":"DEGREES(ACOS((COS(RADIANS(I15*2))-COS(RADIANS(I13*2))*COS(RADIANS(I14*2)))/(SIN(RADIANS(I13*2))*SIN(RADIANS(I14*2)))))","v":61.868345143961839},"C"]

{"sheet":"nex112_8_4","index":12,"n_rows":14,"n_cols":11,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["geo_4 = nex_112_(8,4) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,5.3961926058912546,9.4146523573721302E-2,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":94.181328044575153},{"$f":"E3*Radius","v":94.146523573721296}]
[26,255,137,6.3056004266257268,0.10999795789323122,180,{"$f":"F4/3","v":60},null,110.05348875977805,109.99795789323122]
[26,88,255,6.6056315769808815,0.11522618035834685,360,120,null,115.29002019202166,115.22618035834685]
[199,255,26,6.6414824440257059,0.11585085105639852,180,60,null,115.91573586164857,115.85085105639851]
[248,26,255,6.8375951860391551,0.11926774558180916,360,120,null,119.33854891489747,119.26774558180917]
[255,154,128,6.8618710550108153,0.11969068270392895,180,60,null,119.76224275723567,119.69068270392894]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",6.8375951860391551,{"$f":"DEGREES(ACOS((COS(RADIANS(I12*2))-COS(RADIANS(I13*2))*COS(RADIANS(I14*2)))/(SIN(RADIANS(I13*2))*SIN(RADIANS(I14*2)))))","v":60.35810840418938},"A"]
[null,null,null,null,null,null,null,"b",6.8375951860391551,{"$f":"DEGREES(ACOS((COS(RADIANS(I13*2))-COS(RADIANS(I14*2))*COS(RADIANS(I12*2)))/(SIN(RADIANS(I14*2))*SIN(RADIANS(I12*2)))))","v":60.35810840418938},"B"]
[null,null,null,null,null,null,null,"c",6.8618710550108153,{"$f":"DEGREES(ACOS((COS(RADIANS(I14*2))-COS(RADIANS(I12*2))*COS(RADIANS(I13*2)))/(SIN(RADIANS(I12*2))*SIN(RADIANS(I13*2)))))","v":60.710641791575121},"C"]

{"sheet":"nex133_9_4","index":13,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["geo_2_3 = nex_133_(9,4) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,4.8717463837453492,8.5002403182362768E-2,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":85.028014718483504},{"$f":"E3*Radius","v":85.002403182362769}]
[26,88,255,5.6991329265211981,9.9427633165353801E-2,180,{"$f":"F4/3","v":60},null,99.468634076614961,99.427633165353797]
[248,26,255,5.9857972525959733,0.10442436669489624,180,60,null,104.47187041463043,104.42436669489624]
[199,255,26,5.9864056754777257,0.10443497119180872,180,60,null,104.48248939716149,104.43497119180873]
[26,255,137,6.0472821487860449,0.10549600177809872,180,60,null,105.54498429339409,105.49600177809872]
[128,135,255,6.236016155485383,0.10878530126443071,90,30,null,108.83901412077859,108.78530126443071]
[128,255,216,6.2406093782986591,0.10886534936129133,180,{"$f":"F9/3","v":60},null,{"$f":"RADIANS(D9)*Radius","v":108.91918098214796},{"$f":"E9*Radius","v":108.86534936129134}]
[255,154,128,6.2436581989042859,0.10891848239086231,180,60,null,108.97239294001881,108.91848239086231]
[197,255,128,6.2646860169352738,0.10928494057717099,180,60,null,109.33939759916977,109.28494057717099]
[255,128,232,6.2999844406580063,0.10990008867344739,180,60,null,109.95547131389553,109.90008867344739]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",5.9864056754777257,{"$f":"DEGREES(ACOS((COS(RADIANS(I16*2))-COS(RADIANS(I17*2))*COS(RADIANS(I18*2)))/(SIN(RADIANS(I17*2))*SIN(RADIANS(I18*2)))))","v":58.644416157603985},"A"]
[null,null,null,null,null,null,null,"b",6.2436581989042859,{"$f":"DEGREES(ACOS((COS(RADIANS(I17*2))-COS(RADIANS(I18*2))*COS(RADIANS(I16*2)))/(SIN(RADIANS(I18*2))*SIN(RADIANS(I16*2)))))","v":62.883378787751226},"B"]
[null,null,null,null,null,null,null,"c",6.0472821487860449,{"$f":"DEGREES(ACOS((COS(RADIANS(I18*2))-COS(RADIANS(I16*2))*COS(RADIANS(I17*2)))/(SIN(RADIANS(I16*2))*SIN(RADIANS(I17*2)))))","v":59.599549811250832},"C"]

{"sheet":"nex133_11_1","index":14,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["geo_3_2 = nex_133_(11,1) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,4.8717463837453385,8.5002403182362782E-2,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":85.02801471848332},{"$f":"E3*Radius","v":85.002403182362784}]
[26,88,255,5.6991329265211901,9.9427633165353746E-2,180,{"$f":"F4/3","v":60},null,99.468634076614819,99.42763316535374]
[248,26,255,5.9857972525959884,0.10442436669489624,180,60,null,104.4718704146307,104.42436669489624]
[199,255,26,5.9864056754777177,0.10443497119180868,180,60,null,104.48248939716134,104.43497119180869]
[26,255,137,6.0472821487860688,0.10549600177809879,180,60,null,105.54498429339451,105.49600177809879]
[128,135,255,6.2360161554853786,0.10878530126443085,90,30,null,108.83901412077851,108.78530126443086]
[128,255,216,6.2406093782986618,0.10886534936129129,180,60,null,{"$f":"RADIANS(D9)*Radius","v":108.91918098214802},{"$f":"E9*Radius","v":108.86534936129129}]
[255,154,128,6.2436581989042859,0.10891848239086234,180,60,null,108.97239294001881,108.91848239086234]
[197,255,128,6.2646860169352747,0.109284940577171,180,60,null,109.33939759916979,109.284940577171]
[255,128,232,6.2999844406580046,0.10990008867344747,180,60,null,109.95547131389549,109.90008867344747]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",5.9857972525959884,{"$f":"DEGREES(ACOS((COS(RADIANS(I16*2))-COS(RADIANS(I17*2))*COS(RADIANS(I18*2)))/(SIN(RADIANS(I17*2))*SIN(RADIANS(I18*2)))))","v":58.654433254740354},"A"]
[null,null,null,null,null,null,null,"b",6.2406093782986618,{"$f":"DEGREES(ACOS((COS(RADIANS(I17*2))-COS(RADIANS(I18*2))*COS(RADIANS(I16*2)))/(SIN(RADIANS(I18*2))*SIN(RADIANS(I16*2)))))","v":62.852741671563834},"B"]
[null,null,null,null,null,null,null,"c",6.0472821487860688,{"$f":"DEGREES(ACOS((COS(RADIANS(I18*2))-COS(RADIANS(I16*2))*COS(RADIANS(I17*2)))/(SIN(RADIANS(I16*2))*SIN(RADIANS(I17*2)))))","v":59.619740272861641},"C"]

{"sheet":"nex147_7_7","index":15,"n_rows":19,"n_cols":11,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["geo_1_4 = nex_147_(7,7) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,4.5884247370496425,8.0061720959200347E-2,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":80.0831191414713},{"$f":"E3*Radius","v":80.061720959200343}]
[26,88,255,5.3706735923188189,9.3701624176814075E-2,180,{"$f":"F4/3","v":60},null,93.735937235875028,93.701624176814079]
[248,26,255,5.6530543063722645,9.862439593170777E-2,180,60,null,98.664410440240289,98.624395931707767]
[199,255,26,5.6537038171271981,9.8635718239976175E-2,180,60,null,98.675746541440986,98.635718239976171]
[26,255,137,5.7107407333553244,9.9629976595805483E-2,180,60,null,99.671228524805983,99.629976595805488]
[128,135,255,5.9057220145444562,0.10302867103492856,180,60,null,103.07429386131321,103.02867103492856]
[197,255,128,5.9089808193565725,0.10308547234893499,180,60,null,{"$f":"RADIANS(D9)*Radius","v":103.13117073496447},{"$f":"E9*Radius","v":103.08547234893499}]
[255,154,128,5.9370306182195689,0.10357437987047236,180,60,null,103.62073207964592,103.57437987047236]
[128,61,13,5.9524362895175642,0.10384289782324839,90,30,null,103.88961176727592,103.84289782324839]
[128,255,216,5.9687324193642564,0.10412693425819744,180,60,null,104.17403288843323,104.12693425819744]
[255,128,232,5.991500245085903,0.10452376679596712,180,{"$f":"F13/3","v":60},null,{"$f":"RADIANS(D13)*Radius","v":104.57140641079621},{"$f":"E13*Radius","v":104.52376679596712}]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",5.9057220145444562,{"$f":"DEGREES(ACOS((COS(RADIANS(I17*2))-COS(RADIANS(I18*2))*COS(RADIANS(I19*2)))/(SIN(RADIANS(I18*2))*SIN(RADIANS(I19*2)))))","v":59.922600772905156},"A"]
[null,null,null,null,null,null,null,"b",5.9524362895175642,{"$f":"DEGREES(ACOS((COS(RADIANS(I18*2))-COS(RADIANS(I19*2))*COS(RADIANS(I17*2)))/(SIN(RADIANS(I19*2))*SIN(RADIANS(I17*2)))))","v":60.703094175402896},"B"]
[null,null,null,null,null,null,null,"c",5.9370306182195689,{"$f":"DEGREES(ACOS((COS(RADIANS(I19*2))-COS(RADIANS(I17*2))*COS(RADIANS(I18*2)))/(SIN(RADIANS(I17*2))*SIN(RADIANS(I18*2)))))","v":60.443658459188832},"C"]

{"sheet":"nex147_11_2","index":16,"n_rows":19,"n_cols":11,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["geo_4_1 = nex_147_(11,2) 2/3",null,null,null,null,null,null,null,"Radius ",1000]
["R","G","B","central angle","unit chord length","count","by 3",null,"Arc","Chord"]
[255,26,26,4.5884247370496434,8.006172095920025E-2,180,{"$f":"F3/3","v":60},null,{"$f":"RADIANS(D3)*Radius","v":80.083119141471329},{"$f":"E3*Radius","v":80.061720959200244}]
[26,88,255,5.3706735923188047,9.3701624176814019E-2,180,{"$f":"F4/3","v":60},null,93.735937235874786,93.701624176814022]
[248,26,255,5.6530543063722529,9.8624395931707784E-2,180,60,null,98.664410440240076,98.624395931707781]
[199,255,26,5.653703817127175,9.863571823997612E-2,180,60,null,98.675746541440589,98.635718239976114]
[26,255,137,5.7107407333553235,9.9629976595805456E-2,180,60,null,99.671228524805969,99.629976595805459]
[128,135,255,5.9057220145444518,0.10302867103492856,180,60,null,103.07429386131312,103.02867103492856]
[255,154,128,5.9089808193565911,0.10308547234893507,180,60,null,{"$f":"RADIANS(D9)*Radius","v":103.1311707349648},{"$f":"E9*Radius","v":103.08547234893507}]
[197,255,128,5.9370306182195742,0.10357437987047231,180,60,null,103.62073207964602,103.57437987047231]
[128,61,13,5.9524362895175713,0.10384289782324857,90,30,null,103.88961176727605,103.84289782324856]
[128,255,216,5.9687324193642954,0.10412693425819763,180,60,null,104.17403288843391,104.12693425819764]
[255,128,232,5.9915002450859109,0.10452376679596712,180,60,null,{"$f":"RADIANS(D13)*Radius","v":104.57140641079634},{"$f":"E13*Radius","v":104.52376679596712}]
[]
[null,null,null,null,null,null,null,null,"Angle calculator"]
[null,null,null,null,null,null,null,null,"central angles","opposite to side"]
[null,null,null,null,null,null,null,"a",5.3706735923188047,{"$f":"DEGREES(ACOS((COS(RADIANS(I17*2))-COS(RADIANS(I18*2))*COS(RADIANS(I19*2)))/(SIN(RADIANS(I18*2))*SIN(RADIANS(I19*2)))))","v":57.03067516035069},"A"]
[null,null,null,null,null,null,null,"b",5.653703817127175,{"$f":"DEGREES(ACOS((COS(RADIANS(I18*2))-COS(RADIANS(I19*2))*COS(RADIANS(I17*2)))/(SIN(RADIANS(I19*2))*SIN(RADIANS(I17*2)))))","v":61.959294467932565},"B"]
[null,null,null,null,null,null,null,"c",5.6530543063722529,{"$f":"DEGREES(ACOS((COS(RADIANS(I19*2))-COS(RADIANS(I17*2))*COS(RADIANS(I18*2)))/(SIN(RADIANS(I17*2))*SIN(RADIANS(I18*2)))))","v":61.947099469500891},"C"]