You will need 3 files (2 of those are programs and 1 is firmware bin file)

1. FCDHID2.002.exe program (that sets FCD Pro into bootloader mode when one can reflash firmware)

http://www.funcubedongle.com/MyImages/FCHid2.002.zip

1. FCHIDBL2.001.exe
2. Firmware file is FCD2.20.03.48.pro.bin

Current firmware (12/03/2018) http://www.funcubedongle.com/MyImages/FCD2.20.03.pro.bin

More information here (lots of guidelines, links to firmware and programs)

<http://www.funcubedongle.com/?page_id=1225>

<http://www.funcubedongle.com/?page_id=313>













